**LCD (liquid crystal display) circuitry**

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **S. No.** | **Components** | **Value** | **No. of components** | **Device** | **Library** | **Sub-library** | **Packaging** |
| 1 | LCD Display 16\*2 | ---------- | 1 | Through hole | display-lcd | TUXGR\_16X2\_R2 | TUXGR\_16X2\_R2 |
| 2 | Potentiometer | 10K | 1 | Through hole | bourns | 3362P (3362) | 3362P |

**Jumper/Connector:**

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **S. No.** | **Jumper** | **No. of pins** | **No. of Jumper** | **Library** | **Sub-library** | **Package** |
| 1 | Jumper1 | 11 | 2 | con-amp-quick | M11 | 11P |